For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Conditioning Accumulator Bracket Bolt | 6 N·m | 53 lb ft
Air Conditioning Accumulator Bolt (At Module) | 16 N·m | 12 lb ft
Air Conditioning Accumulator Hose Bracket Nut ( At Strut Tower) | 8 N·m | 71 lb in
Air Conditioning Compressor and Condenser Hose Bolt (At Accumulator) | 16 N·m | 12 lb ft
Air Conditioning Compressor and Condenser Hose Nut (At Condenser) | 16 N·m | 12 lb ft
Air Conditioning Compressor and Condenser Hose Bolt (At Compressor) | 33 N·m | 24 lb ft
Air Conditioning Compressor Bracket Bolt (3.8L VIN K) | 30 N·m | 22 lb ft
Air Conditioning Compressor Bracket Bolt (3.8L VIN K) | 50 N·m | 37 lb ft
Air Conditioning Compressor Bracket Bolt (5.7L VIN G) | 50 N·m | 37 lb ft
Air Conditioning Compressor Bolt (5.7L VIN G) | 50 N·m | 37 lb ft
Air Conditioning Compressor Bolt (3.8L VIN K) | 50 N·m | 37 lb ft
Air Conditioning Compressor Rear Bolt (3.8L VIN K) | 30 N·m | 22 lb ft
Air Conditioning Compressor Refrigerant Pressure Sensor | 6 N·m | 53 lb in
Air Conditioning Evaporator and Blower Upper Case Bolt | 1.8 N·m | 16 lb in
Air Conditioning Evaporator Bracket Bolt | 2.0 N·m | 18 lb in
Air Conditioning Evaporator Tube Bolt (At Module) | 16 N·m | 12 lb ft
Air Conditioning Evaporator Tube Bolt (At Condenser) | 16 N·m | 12 lb ft
Air Distributor Duct Bolt | 2.2 N·m | 19 lb in
Bi-Level Mode Valve Linkage Bolt | 2.3 N·m | 20 lb in
Blower Motor Bolt | 2.3 N·m | 20 lb in
Blower Motor Resistor Bolt | 2 N·m | 18 lb in
Front Floor Air Duct Bolt | 1.9 N·m | 17 lb in
HVAC Control Bolt | 2.2 N·m | 19 lb in
Heater Core Clamp Bolt | 1.8 N·m | 16 lb in
Heater Core Tube Clamp Bolt | 2.0 N·m | 18 lb in
Heater Module Screw | 1.8 N·m | 16 lb in
Heater Hose Bracket Bolt | 14 N·m | 10 lb ft
I/P Outer Air Outet Duct Bolt | 2.2 N·m | 19 lb in
Negative Battery Cable Nut to Engine Block Stud (3.8L VIN K) | 25 N·m | 18 lb ft
Temperature Control Cable Bolt | 1.9 N·m | 17 lb in
Temperature Valve Shroud Case Bolt | 2.0 N·m | 18 lb in
Vacuum Tank Mounting Bolt | 2.5 N·m | 22 lb in