For 1990-2009 cars

# SMU-SEC. 8E -REVISED WIPER ARM TORQUE

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 8E - REVISED WIPER ARM TORQUE NUT SPECIFICATIONS

#### MODELS: 1998 CHEVROLET CAMARO 1998 PONTIAC FIREBIRD

THIS BULLETIN IS BEING ISSUED TO REVISED THE WIPER TORQUE NUT SPECIFICATIONS IN SECTION 8E OF THE SERVICE MANUAL AS FOLLOWS:

O ON PAGE 8E-11 UNDER "WIPER ARM REPLACEMENT - INSTALL OR CONNECT"

- CHANGE FROM: "TIGHTEN NUT(7) TO 32 N.M (24 LB FT) WHILE HOLDING WIPER ARM"

- CHANGE TO: "TIGHTEN NUT(7) TO 23 N.M (17 LB FT) WHILE HOLDING WIPER ARM"

O ON PAGE 8E-11, IN FIGURE 9 - "WIPER ARM NUT REMOVAL"

- CHANGE FROM: "7 NUT, 32 N.M (24 LB FT)"

- CHANGE TO: "7 NUT, 23 N.M (17 LB FT)"

O ON PAGE 8E-18 UNDER "FASTENER TIGHTENING SPECIFICATIONS"

- CHANGE FROM: "WIPER ARM NUTS (7) . . . . . 32 N.M (24 LB FT)"

- CHANGE TO: "WIPER ARM NUTS (7) . . . . . 23 N.M (17 LB FT)"

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.