For 1990-2009 cars

#### Instrument Cluster

Connector Part Information |

• | 12065803

• | 34-Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | PNK | 39 | Power feed from gages Fuse 9
A2 | DK BLU | 1936 | Fuel gage signal
A3 | GRY | 728 | SECURITY indicator lamp control
A4 | BRN/WHT | 419 | SERVICE ENGINE SOON indicator lamp control
A5 | PNK | 39 | Power feed from gages Fuse 9
A6 | YEL/BLK | 68 | Low coolant level indicator control
A7 | BRN | 358 | AIR BAG indicator control
A8 | PPL/WHT | 1572 | TCS OFF indicator control (with NW9)
A10 | TAN/WHT | 33 | BRAKE warning indicator lamp control
A11 | LT GRN | 11 | High beam headlights on
A12 | PPL/WHT | 237 | FASTEN SEATBELT indicator lamp control
A13 | ORN | 640 | Power feed from PWR ACCY Fuse 7
A14 | RED | 225 | Generator output indicator control
A15 | BRN/WHT | 1173 | Oil level lamp signal
A16 | DK BLU | 1537 | LOW TRAC indicator lamp control
A17 | DK GRN | 135 | Coolant temperature sensor signal
B1 | BRN | 9 | Odometer illumination
B2 | GRY | 8 | IP illumination lamps feed
B3 | BLK | 650 | Ground
B4 | WHT | 375 | SKIP SHIFT indicator lamp control (V8 only)
B5 | DK BLU/WHT | 1415 | Right turn signal switch output
B12 | DK GRN/WHT | 817 | Vehicle speed signal-4000 pulses per mile
B13 | WHT | 121 | Tachometer signal
B14 | LT BLU/WHT | 1414 | Left turn signal switch output
B15 | BLK/WHT | 451 | Ground
B16 | TAN | 31 | Oil pressure indicator control
B17 | LT GRN | 867 | ABS fail signal