For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire Headlamp Leveling System Check performed? | -- | Go to Step 2 | Go to Headlight Leveling System Check
2 |

1. Place the headlamp switch in the HEAD position.
2. Visually verify that the headlamps are operative.
3. Adjust the IP dimmer switch to a mid-range position.
4. Disconnect the connector at the headlamp leveling switch.
5. Connect a test light between cavities 7 and 6 of the headlamp leveling switch connector.

Did the test light illuminate?

--

Go to Step 3

Go to Step 4

3 | Replace the headlamp leveling switch. Refer to Headlamp Leveling Switch Replacement. Is the repair complete? | -- | Go to Step 5 | --
4 | Repair the poor connection or open in circuit 650. Is the repair complete? | -- | Go to Step 5 | --
5 |

1. Turn the ignition switch to the OFF position.
2. Reconnect all connectors/components removed.

Have all repairs been made?

--

Go to Headlight Leveling System Check

--