For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Important: Use a reliable torque wrench in order to tighten the parts listed. A reliable torque wrench will ensure proper tightening of the parts without straining or distorting the parts. The following specifications are for clean and lightly-lubricated threads only. Dry or dirty threads produce increased friction. Friction prevents the measurement of tightness.
Differential Carrier Bearing Cap Bolt/Screw | 75 N·m | 55 lb ft
Differential Drive Pinion Gear Setting Gauge Nut | 2.3 N·m | 20 lb in
Differential Pinion Gear Shaft Lock Bolt/Screw | 36 N·m | 27 lb ft
Differential Ring Gear Bolt/Screw | 120 N·m | 89 lb ft
Rear Axle Housing Cover Bolt/Screw | 30 N·m | 22 lb ft
Rear Axle Housing Drain Plug | 35 N·m | 26 lb ft
Sensor Plug Mounting Bolt/Screw | 10 N·m | 89 lb in
Wheel Bolt | 140 N·m | 100 lb ft
Wheel Speed Sensor Mounting Plug | 10 N·m | 89 lb in