For 1990-2009 cars

# INFORMATION ON MIRROR APPLIQUE CHANGES

#### SUBJECT: INFORMATION ON MIRROR APPLIQUE CHANGES

#### MODELS: 1994-95 CHEVROLET CAMARO 1994-95 PONTIAC FIREBIRD

1994 VIN'S WITH NEW APPLIQUES; - CHEVROLET VIN'S R2 223072 THROUGH R2 223088 - PONTIAC VIN'S R2 250757 THROUGH R2 250764

1995 CHEVROLET CAMARO S2225952 1995 PONTIAC FIREBIRD S2225352

SOME 1994-95 CAMARO AND FIREBIRD MODELS HAVE A DIFFERENT MIRROR APPLIQUE THAN PREVIOUS (1993, 1994) MODELS. THE NEW PART NUMBERS ARE:

10273041 - RIGHT SIDE 10273042 - LEFT SIDE

THESE NEW PARTS WILL HAVE A LIP ON THE UPPER OUTER EDGE OF THE APPLIQUE FOR ENHANCED WATERLEAK PERFORMANCE.

IN ADDITION TO THE LIP CHANGE, THE FRONT BELT OPENING SEAL WILL NOW ATTACH TO THE APPLIQUE WITH A SMALL PLASTIC FASTENER, FOR ENHANCED WINDNOISE PERFORMANCE.

THE NEW PART NUMBERS FOR THE FRONT BELT OPENING SEALS ARE:

10270466 - RIGHT SIDE 10270467 - LEFT SIDE

THE NEW PARTS CAN BE USED ON PAST MODEL (1993-94) VEHICLES.

#### PART AVAILABILITY:

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE: NEW LABOR OPERATION: B4090 RIGHT B4091 LEFT

NEW LABOR OPERATION TIME: 0.5 HRS.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.