For 1990-2009 cars

# DISABLED VEHICLE TOWING, NEW PROCEDURE FOR REAR WHEEL TOW

#### SUBJECT: DISABLED VEHICLE TOWING

#### VEHICLES AFFECTED: 1991 PONTIAC F-CAR (FIREBIRD, FORMULA, GTA, TRANS AM)

The 1991 Pontiac Firebird, Formula, GTA, and Trans Am rear towing procedure has changed.

The 1991 General Motors Passenger Car and Light Duty Truck Towing Manual (T-62) does not state the following change:

The 1991 Pontiac Firebird, Formula, GTA and Trans Am MUST NOT be towed from the rear with sling-type towing equipment. Use either wheel-lift or car carrier equipment to transport this vehicle.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.