For 1990-2009 cars

### Removal Procedure

1. Remove cargo compartment side trim panel (drivers-side only). Refer to Cargo Area Side Trim Panel Replacement .
2. Remove left section (1) of rear compartment trim panel carpet. (felt liner at rear).
3. Remove luggage screen support bolt/screw from support (2).
4. Remove support (2) from vehicle body (3).

### Installation Procedure

1. Install support (2) to vehicle body (3).
2. Install luggage screen support bolt/screw to support (2).

Tighten
Tighten the bolt/screw to 6 N·m (53 lb in).

3. Install left section (1) of rear compartment trim panel carpet into original position (felt liner at rear).
4. Install cargo compartment side trim panel (drivers-side only). Refer to Cargo Area Side Trim Panel Replacement .