For 1990-2009 cars

## Cargo Area Front Trim Panel Replacement Convertible

### Removal Procedure

1. Lower the seatback.
2. Remove the left or right shroud side trim finishing panel.
3. Remove the coat hook (coupe only).

Important: Release retainer with a screwdriver and pull out if necessary.

4. Remove the rear seat striker bolt/screw and washer.
5. Remove quarter inner trim finish panel extension bolt/screw (1) (convertible only).
6. Remove quarter inner trim finish panel extension (2) (convertible only).
7. Remove quarter inner trim finishing panel

Important: Push lap belt through slot in quarter inner trim finishing panel.

8. Remove speaker grille, if replacing panel.
9. Disconnect and remove quarter courtesy lamp (convertible only) if replacing panel.

### Installation Procedure

1. Install and connect quarter courtesy lamp (convertible only) if removed.
2. Install speaker grille, if removed.
3. Install quarter inner trim finishing panel

Important: Thread lap belt through slot in quarter inner trim finishing panel.

4. Install quarter inner trim finish panel extension (convertible only) (2).
5. Install quarter inner trim finish panel extension bolt/screw (1) (convertible only).

Tighten
Tighten the screws to 1.9 N·m (17 lb in).

6. Install the rear seat striker bolt/screw and washer.

Tighten
Tighten the bolt to 35 N·m (26 lb in).

7. Install the coat hook (coupe only).

Important: Slide into position and press retainer to lock.

8. Install the left or right shroud side trim finishing panel.
9. Raise the seatback.

## Cargo Area Front Trim Panel Replacement Coupe

### Removal Procedure

1. Lower the seatback.
2. Remove the left or right shroud side trim finishing panel.
3. Remove the coat hook (coupe only).

Important: Release retainer with a screwdriver and pull out if necessary.

4. Remove the rear seat striker bolt/screw and washer.
5. Remove quarter inner trim finishing panel (1) from vehicle body (2).

Important: Push lap belt through slot in quarter inner trim finishing panel.

6. Remove speaker grille, if replacing panel.

### Installation Procedure

Important: Thread lap belt through slot in quarter inner trim finishing panel.

1. Install speaker grille, if removed.
2. Install quarter inner trim finishing panel (1) to vehicle body (2).
3. Install the rear seat striker bolt/screw and washer.

Tighten
Tighten the bolt to 35 N·m (26 lb in).

4. Install the coat hook (coupe only).

Important: Slide into position and press retainer to lock.

5. Install the left or right shroud side trim finishing panel.
6. Raise the seatback.