For 1990-2009 cars

### Removal Procedure

1. Remove the front end fascia outer deflector bolts (2) from the following components:

• | The front fascia

• | The front bumper fascia lower deflector (1)

2. Remove the front end fascia outer deflector (1) from the vehicle.

### Installation Procedure

1. Install the front end fascia outer deflector (1) to the vehicle.
2. Install the front end fascia outer deflector bolts (2) to the following components:

• | The front fascia

• | The front bumper fascia lower deflector (1)

Tighten
Tighten the front end fascia outer deflector bolts (2) to 10 N·m (89 lb in).