For 1990-2009 cars

# LABOR TIME GUIDE REQUEST FOR REVIEW UPDATES

This bulletin addresses changes to the published Pontiac Labor Time Guide for September, October, November, December and January, 1989 changes attached. These changes are the result of dealer "Requests For Review" being handled by C-P-C Technical Service Activity.

These updates will be included in future revisions as printed, and at that time it is recommended that you discard the paper copy. In the case of past model year updates, it is recommended that this bulletin be retained with the appropriate model year labor time guide as a complete revision will not be provided.

Request For Review

Operation Vehicles Series Operation Description Number A B F G H J N P T Vin Code

Sunshade, sunroof B2900 .4 sliding glass panel - R&R or replace Note: applicable model year: 1988

Cover and/or gasket, rocker-replace Note: applicable model years: 1982/87 w/3.8L Both banks J0307 .9

Pump and/or gasket, coolant-replace J3480 1.8 Note: applicable model years: 1985-87 w/V-6

REQUEST FOR REVIEW VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N T W NUMBER VIN CODE

FILLER, FRONT BUMPER - R & R OR REPLACE NOTE: Applicable model years: 1988-89 RIGHT B0500 .3 LEFT B0501 .3

LATCH, VISTA VENT GLASS - B2200 .3 ALIGN OR REPLACE NOTE: Applicable model year: 1989

RETAINER, VISTA VENT - REPLACE B2215 .4 NOTE: Applicable model year: 1989

HINGE, VISTA VENT GLASS - R&R OR REPLACE NOTE: Applicable model year: 1989 RIGHT B2220 .2 LEFT B2221 .2

AIR DEFLECTOR, ROOF OPENING B2230 .4 - REPLACE NOTE: Applicable model year: 1989

GLASS, VISTA VENT - REPLACE B2240 .2 NOTE: Applicable model year: 1989

ESCUTCHEON, VISTA VENT-REPLACE B2245 .2 NOTE: Applicable model year: 1989

LACE, VISTA VENT OPENING B2250 .2 FINISHING - REPLACE NOTE: Applicable model year: 1989 ADD: A- To Color Coat .2 GB

FRAME, VISTA VENT - REPLACE B2278 2.8 NOTE: Applicable model year: 1989

GUIDE, SUNROOF SLIDING PANEL B2840 1.9 SIDE - R&R OR REPLACE NOTE: Applicable model years: 1987-89

MOLDING AND/OR OUTER STRIP, FRONT DOOR WINDOW REVEAL - R&R OR REPLACE NOTE: Applicable model years: 1988-89 RIGHT B7840 .5 LEFT B7841 .5

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N T W NUMBER VIN CODE

ASH TRAY, BODY (EXCEPT I.P. & CONSOLE) - REPLACE NOTE: Applicable model years: 1988-89 RIGHT C3960 .2 LEFT C3961 .2

BLADDER ASSEMBLY, PNEUMATIC SEAT - REPLACE NOTE: Applicable model years: 1988-89 LUMBAR SEAT BACK PASSENGER C7070 .8 DRIVER C7071 .8 PASSENGER SEAT BACK CONTOUR RIGHT C7074 .8 LEFT C7075 .8 DRIVER SEAT BACK CONTOUR RIGHT C7076 .8 LEFT C7077 .8 RELAY - REPLACE NOTE: Applicable model years: 1988-89 CONDENSER FAN MOTOR D1040 .2

A/C SYSTEM - LEAK TEST D3000 .4 .4 .4 .4 .4 .4 .4 .4 DISCHARGES SYSTEM NOTE: Applicable model year: 1989

PULLEY, COMPRESSOR BELT IDLER D4005 .5 - REPLACE NOTE: Applicable model years: 1987-88

BRACKEL COMPRESSOR BELT IDLER D4010 .6 PULLEY - REPLACE NOTE: Applicable model years: 1987-88

SENSOR, WHEEL SPEED - REPLACE NOTE: Applicable model year: 1989 FRONT RIGHT H2410 .7 LEFT H2411 .7 BOTH H2412 .9 REAR RIGHT H2414 .9 LEFT H2415 .9 BOTH H2417 1.2

ACCUMULATOR ASSEMBLY, (ABS) H2474 .6 - REPLACE NOTE: Applicable model year: 1989

REQUEST FOR REVIEW

VEHICLES SERIES OPERATION DESCRIPTION OPERATION A B F H J N T W NUMBER VIN CODE

RELAY, PUMP (ABS) - REPLACE H2475 .3 NOTE: Applicable model year: 1989

HOSE, LOW PRESSURE (ABS) H2477 .6 - REPLACE NOTE: Applicable model year: 1989

VALVE, PRESSURE RELIEF (ABS) H2479 .5 - REPLACE NOTE: Applicable model year: 1989

HOSE, HIGH PRESSURE (ABS) H2481 .7 - REPLACE NOTE: Applicable model year: 1989

RESERVOIR - REPLACE H2489 .8 NOTE: Applicable model year: 1989 w/ ABS

RELAY, ENABLE (ABS) - REPLACE NOTE: Applicable model year: 1989 FRONT H2491 .2 REAR H2492 .3

SENSOR, FLUID LEVEL - REPLACE H2493 .2 NOTE: Applicable model year: 1987 H series; 1989 W series

SWITCH, PRESSURE(ABS) - REPLACE H2494 .6 NOTE: Applicable model year: 1989

PUMP AND MOTOR ASSEMBLY, H2498 1.6 (ABS) - REPLACE NOTE: Applicable model year: 1989

MODULE, ELECTRONIC BRAKE H2500 .4 CONTROL (ABS) - REPLACE NOTE: Applicable model year: 1989

HYDRAULIC UNIT (ABS) - H2518 1.5 R&R OR REPLACE NOTE: Applicable model year: 1989 NOTE: Referred to as Powermaster III

SOLENOID (ABS) - REPLACE NOTE: Applicable model year: 1989 ONE H2526 1.0 ALL H2527 1.1

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F J K M T W MUMBER VIN CODE

HARNESS, WHEEL SPEED SENSOR JUMPER WIRING (ABS) - REPLACE NOTE: Applicable model year: 1989 FRONT RIGHT H2530 .9 LEFT H2531 .9 BOTH H2532 1.3 REAR RIGHT H2534 .7 LEFT H2535 .6 BOTH H2537 .7

HARNESS, POWERMASTER III H2538 .4 WIRING (ABS) - REPLACE NOTE: Applicable model year: 1989

DIODE, (ABS) - REPLACE H2545 .3 NOTE: Applicable model year: 1989

FUSE AND/OR FUSE ELEMENT, (ABS) H2547 .3 - REPLACE NOTE: Applicable model year: 1989

CONTROL ASSEMBLY, PARKING BRAKE H2840 .8 - REPLACE NOTE: Applicable model year: 1988

BELT, DRIVE - ADJUST NOTE: Applicable model years: 1988-89 w/Quad 4 P/S J0656 .2

MOUNT, ENGINE - REPLACE NOTE: Applicable model years: 1985-87 w/V-6 FRONT J1502 .6 REAR J1503 .7

ENGINE, PARTIAL/BASIC - REPLACE J1820 11.3 NOTE: Applicable model years: 1986-89 w/port injection

PUMP AND/OR GASKET, COOLANT J3480 2.0 - REPLACE NOTE: Applicable model years: 1987-89 w/OHC-4 ADD: A- With A/C .3

SENSOR, CRANKSHAFT - REPLACE J4355 .8 NOTE: Applicable model years: 1985-87 w/V-6

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N T W NUMBER VIN CODE

SOLENOID, STARTER MOTOR - REPLACE J4580 1.8 NOTE: Applicable model years: 1987-89 w/2.0L

DRIVE ASSEMBLY, STARTER MOTOR J4600 2.0 - REPLACE NOTE: Applicable model years: 1987-89 w/2.0L

MOTOR ASSEMBLY, STARTER - R&R J4620 1.8 NOTE: Applicable model years: 1987-89 w/2.0L

MOTOR ASSEMBLY, STARTER - REPLACE J4640 1.8 NOTE: Applicable model years: 1987-89 w/2.0L

VALVE, IDLE AIR CONTROL - REPLACE J5542 .7 NOTE: Applicable model years: 1985-87 w/V-8 PFI

SWITCH - REPLACE NOTE: Applicable model years: 1988-89 SEAT LUMBAR CONTROL ADJUST RIGHT N2416 .2 LEFT N2417 .2

RELAY - REPLACE NOTE: Applicable model years: 1988-89 THEFT DETERRENT INTERRUPT N2910 .4 PARK/TURN SIGNAL N2923 .2

MOTOR - REPLACE NOTE: Applicable model years: 1988-89 SUNROOF OR ASTRO ROOF DRIVE N3360 1.0

INSTRUMENT PANEL CLUSTER COMPONENTS (DIGITAL/ELECTRONIC) - REPLACE NOTE: Applicable model years: 1988-89 MODULE, PRNDL DECODER N4175 .5 COMPASS N4185 .4

MODULE - REPLACE COMPASS N4819 .4 NOTE: Applicable model years: 1988-89 HEADLAMP CLOSURE PANEL N4829 .3 NOTE: Applicable model years: 1987-89

REQUEST FOR REVIEW VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N T W NUMBER

WIRING AND/OR CONNECTOR - REPAIR NOTE: Applicable model years: 1988-89 ANTI-LOCK BRAKING SYSTEM N6035 .5

SPEAKER, RADIO - REPLACE NOTE: Applicable model years: 1988-89 REAR RIGHT R0950 .6 LEFT R0951 .6

LUGGAGE RACK COMPONENTS - REPLACE NOTE: Applicable model years: 1988-89 BRACKET AND/OR BAR R2320 .5

THEFT DETERRENT SYSTEM COMPONENTS - REPLACE NOTE: Applicable model years: 1988-89 CONTROLLER R2820 .3

CABLE ASSEMBLY, MANUAL FUEL FILLER DOOR LOCK RELEASE - REPLACE R4085 .6 NOTE: Applicable model years: 1988-89

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.