For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 |

1. Turn the ignition switch to the RUN position.
2. Place the multi-function lever in the left turn position.
3. Observe the left front park/turn lamp.

Does the left turn signal operate?

--

Go to Step 2

Go to Exterior Lights

2 |

1. Remove the instrument cluster.
2. Connect a test lamp from the instrument cluster connector terminal A12 to ground.
3. Turn the ignition switch to the RUN position.
4. Place the multi-function lever in the left turn position.

Does the test lamp blink on then off?

--

Go to Step 3

Go to Step 4

3 |

1. Check for a poor connection at the instrument cluster terminal A12.
2. If the connection is OK, replace the instrument cluster. Refer to Instrument Cluster Replacement .

Is the repair complete?

--

System OK

--

4 | Repair the open in circuit 1414 (USA or Gulf States) or circuit 14 (Europe or Japan). Is the repair complete? | -- | System OK | --