For 1990-2009 cars

### Removal Procedure

1. Remove the clip (1) from the instrument panel tie bar.
2. Disconnect the turn signal flasher (2) electrical connector (3).
3. Remove the clip (1) from the turn signal flasher (2).

### Installation Procedure

1. Install the clip (1) to the turn signal flasher (2).
2. Connect the turn signal flasher (2) electrical connector (3).
3. Install the clip (1) to the instrument panel tie bar.