For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to SECTION 0A.
2. Relieve drive belt tension. Use a socket with a handle on the tensioner pulley bolt in order to push the tensioner downward.
3. Remove the drive belt.

### Installation Procedure

1. Relieve drive belt tension. Use a socket with a handle on the tensioner pulley bolt in order to push the tensioner downward.

Important: Ensure that the drive belt is aligned into the proper groove of each pulley.

2. Install the drive belt.
3. Connect the negative battery cable.