For 1990-2009 cars

### Removal Procedure

1. Position a hex-head socket on the belt tensioner pulley bolt.
2. Rotate the drive belt tensioner (2) clockwise to relieve the tension on the drive belt (1).
3. Remove the drive belt (1) from the tensioner (2) and pulleys.
4. Clean and inspect the belt surfaces of all the pulleys.

### Installation Procedure

1. Route the drive belt (1) around the pulleys.
2. Position a hex-head socket on the belt tensioner pulley bolt.
3. Rotate the drive belt tensioner (2) clockwise to relieve the tension.
4. Install the drive belt (1) onto the drive belt tensioner (2).
5. Inspect the drive belt (1) to ensure that the bolt is properly aligned into the grooves of the pulleys.