For 1990-2009 cars

### Chevrolet Tailpipe Clearance

Measure the clearance from rear fascia line (1) to the tailpipe extension line (2).

Specification
Clearance specification should 40.0 mm (+/- 5.0 mm), 1.575 in (+/- 0.197 in).

### Pontiac Tailpipe Clearance

Measure the clearance from the rear fascia line (1) to the tailpipe extension line (2).

Specification
Clearance specification should be 30.0 mm (+/- 5.0 mm), 1.181 in (+/- 0.197 in).