For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 5A BRAKE MASTER CYLINDER

#### SUBJECT: SECTION SA BRAKE MASTER CYLINDER (REVISED TORQUE SPECIFICATION)

#### VEHICLES AFFECTED: 1993 "F" MODELS

#### APPLICATION:

-----------

1993 Chevrolet Camaro and Pontiac Firebird F-Cars

This update is to identify a change to the brake master cylinder nut torque specification. In the 1993 F-Car Service Manuals, the torque specification was published at 43 N.m (32 lb. ft.). The revised torque is now 32 N.m (24 lb. ft.). Please note this in your Service Manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.