For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 41778-1 Pump Body Bushing Installer/Remover

• | J 41778-2 Pump Body Bushing Position Stop

1. Inspect the oil pump body for the following defects:

• | Worn or damaged bushings

• | Foreign material or debris

• | Porosity

• | Scored or irregular mating faces

• | Cross channel leaks

• | Ring groove damage

2. Remove the front helix retainer (244).
3. Remove the oil seal assembly (243).
4. Using the J 41778-1 with an arbor press, remove the pump body bushing (242).
5. Using J 41778-1 with an arbor press, install a new pump body bushing (242).
6. Use the J 41778-2 to ensure proper bushing depth.