For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 34730-1A Fuel Pressure Gauge

• | J 39765 Fuel Sender Lock Nut Wrench

• | J 42960-1 Fuel Tank Drain Hose

• | J 42960-2 Fuel Flapper Door Holder

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Relieve the fuel system pressure. Refer to the Fuel Pressure Relief Procedure .
3. Drain the fuel tank. Refer to Fuel Tank Draining .
4. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
5. Remove the fuel fill pipe shield.
6. Remove the fuel tank fill pipe support bracket bolt.
7. Remove the exhaust system from the catalytic converter back. Refer to Muffler Replacement in Engine Exhaust.
8. Remove the exhaust pipe heat shield and the exhaust muffler heat shield. Refer to Exhaust Pipe and Muffler Heat Shields Replacement in Engine Exhaust.
9. Clean all fuel pipe connections and surrounding areas before disconnecting the fuel pipes in order to avoid possible contamination of the fuel system.
10. Disconnect the fuel return pipe (2) at the rear quick-connect fitting.
11. Disconnect the EVAP purge pipe (1) at the rear quick-connect fitting.
12. Disconnect the fuel feed pipe at the fuel filter inlet.
13. Cap the fuel pipes in order to prevent possible fuel system contamination.
14. Remove the rear pipe clip.
15. Disconnect the fuel sender and the fuel pressure sensor electrical connectors at the pass through connector.
16. With the aid of an assistant, support the fuel tank.

Notice: Do not bend the fuel tank straps. Bending the fuel tank straps may damage the straps.

17. Remove the fuel tank strap attaching bolts from the underbody brackets.
18. Lower the fuel tank straps.
19. Remove the fuel tank.
20. Place the fuel tank in a suitable work area.
21. Disconnect the hose from the EVAP canister vent solenoid.
22. Remove the EVAP canister vent solenoid from the fuel tank bracket.
23. Disconnect the fill limiter vent valve pipe from the EVAP canister.
24. Carefully bend the fuel tank bracket in order to remove the EVAP canister.
25. Disconnect the fuel feed pipe (4), the fuel return pipe (2), and the EVAP pipe (3) from the fuel sender.
26. Disconnect the EVAP pipe from the fill limiter vent valve pipe (10).
27. Remove the fuel and EVAP pipes from the fuel tank.
28. Disconnect the fuel sender electrical connectors (1).
29. Remove the fuel sender electrical harness (8) from the fuel tank.
30. Remove the fuel sender assembly from the fuel tank. Refer to Fuel Sender Assembly Replacement .
31. Remove the fuel fill hose to fuel tank clamp (1).
32. Remove the fuel fill pipe and hose from the fuel tank.

### Installation Procedure

1. Install the fuel fill pipe and hose to the fuel tank.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Tighten
Tighten the fuel fill hose clamp (1) to 2.5 N·m (22 lb in).

2. Install the fuel sender assembly to the fuel tank. Refer to Fuel Sender Assembly Replacement .
3. Perform the fuel tank leak check. Refer to Fuel Tank Leak Check .
4. Install the fuel sender electrical harness (8) to the fuel tank.
5. Connect the fuel sender electrical connectors (1).
6. Install the fuel feed pipe (4) and the fuel return pipe (2) to the fuel sender and the fuel tank clips.
7. Connect the EVAP pipe (3) to the fuel sender.
8. Connect the EVAP pipe to the fill limiter vent valve pipe (10).
9. Carefully bend the fuel tank bracket in order to install the EVAP canister.
10. Connect the fill limiter vent valve pipe to the EVAP canister.
11. Install the EVAP canister vent solenoid to the fuel tank bracket.
12. Connect the hose to the EVAP canister vent solenoid.
13. With the aid of an assistant, position and support the fuel tank.
14. Position the fuel tank straps up.
15. Install the fuel tank strap attaching bolts.

Tighten
Tighten the fuel tank strap attaching bolts to 33 N·m (24 lb ft).

16. Connect the fuel sender and the fuel pressure sensor electrical connectors at the pass through connector.
17. Remove the caps from the fuel pipes.
18. Connect the fuel feed pipe at the fuel filter inlet.
19. Connect the EVAP purge pipe (1) at the rear quick-connect fitting.
20. Connect the fuel return pipe (2) at the rear quick-connect fitting.
21. Install the fuel and EVAP pipes into the pipe clip.
22. Align the fuel and EVAP pipes into a flat position.
23. Install the pipe clip bolt.

Tighten
Tighten the pipe clip bolt to 5.5 N·m (49 lb in).

24. Install the fuel tank fill pipe support bracket bolt.

Tighten
Tighten the fuel tank fill pipe support bracket bolt to 10 N·m (89 lb in).

25. Install the exhaust system heat shields and attaching screws. Refer to Exhaust Pipe and Muffler Heat Shields Replacement in Engine Exhaust.
26. Install the exhaust system. Refer to Muffler Replacement in Engine Exhaust.
27. Install the fuel filler pipe shield.
28. Lower the vehicle.
29. Refill the fuel tank.
30. Install the fuel filler cap.
31. Connect the negative battery cable.
32. Inspect for leaks.

32.1. | Turn the ignition switch ON for 2 seconds.

32.2. | Turn the ignition switch OFF for 10 seconds.

32.3. | Turn the ignition switch ON.

32.4. | Check for fuel leaks.

33. Perform the idle learn procedure. Refer to PCM Idle Learn Procedure .