For 1990-2009 cars

# ELIMINATE 4TH CLUTCH-700R4-TS PRESSURE SWITCH NOT REQUIRED

#### VEHICLES AFFECTED: 1985 'B' Series Equipped With THM 700-R4 (Code TS Police Option) Transmission

Beginning April 28, 1984, Julian date 119 the 4th clutch switch was eliminated on all 1984 TS model THM 700-R4 transmissions and replaced with a pipe plug. Refer to figures 1 and 2 for switch location.

The 4th clutch switch is not required for this model transmission and was never used. Therefore the switch was eliminated.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.