For 1990-2009 cars

### Removal Procedure

1. Remove the I/P carrier. Refer to Instrument Panel Carrier Replacement in Instrument Panel, Gauges and Console.
2. Place the I/P carrier face down on a clean work surface.
3. Remove the air distributor duct bolts.
4. Remove the air distributor from the I/P carrier.

### Installation Procedure

1. Install the air distributor to the I/P carrier.
2. Install the air distributor duct bolts.

Tighten
Tighten the air distributor duct bolts to 2.2 N·m (19 lb in).

3. Install the I/P carrier. Refer to Instrument Panel Carrier Replacement in Instrument Panel, Gauges and Console.