For 1990-2009 cars

## Generator Bracket Replacement 3.8L

### Removal Procedure

1. Remove generator rear brace. Refer to Generator Brace Replacement .
2. Remove the fuel rail from the upper intake manifold. Refer to Fuel Injection Fuel Rail Assembly Replacement in Engine Controls - 3.8L.
3. Remove the generator brace bracket bolts.
4. Remove the generator bracket from the cylinder head.

### Installation Procedure

1. Install the generator bracket to the cylinder head.
2. Install the generator brace bracket bolts.

Tighten
Tighten the generator brace bracket bolts to 50 N·m (37 lb ft).

3. Install the fuel rail to the upper intake manifold. Refer to Fuel Injection Fuel Rail Assembly Replacement in Engine Controls - 3.8L.
4. Install the generator rear brace. Refer to Generator Brace Replacement .