For 1990-2009 cars

## Drive Belt Tensioner Replacement Accessory

### Removal Procedure

1. Remove the accessory drive belt. Refer to Drive Belt Replacement .
2. Remove the drive belt tensioner bolts.
3. Remove the drive belt tensioner.

### Installation Procedure

1. Install the drive belt tensioner.
2. Install the drive belt tensioner bolts.

Tighten
Tighten the drive belt tensioner bolts to 50 N·m (37 lb ft).

3. Install the accessory drive belt. Refer to Drive Belt Replacement .

## Drive Belt Tensioner Replacement A/C

### Removal Procedure

1. Remove the air conditioning (A/C) drive belt. Refer to Drive Belt Replacement .
2. Remove the A/C drive belt tensioner bolt (3).
3. Remove the A/C drive belt tensioner (4).

### Installation Procedure

1. Install the A/C drive belt tensioner (4).

Important: Be sure the tensioner is fully seated against the compressor bracket before tightening the bolt.

2. Install the A/C drive belt tensioner bolt (3).

Tighten
Tighten the A/C drive belt tensioner bolt (3) to 25 N·m (18 lb ft).

3. Install the A/C drive belt. Refer to Drive Belt Replacement .