For 1990-2009 cars

# INADEQUATE HEATER OUTPUT ON PASSENGER SIDE

INADEQUATE HEATER OUTPUT ON THE PASSENGER SIDE OF SOME 1982 'F' MODELS MAY BE CAUSED BY A MISPOSITIONED R.H. HUSH PANEL. THE FRONT EDGE OF THE HUSH PANEL MUST BE POSITIONED ABOVE THE DASH STUD (PAGES 8C-3 AND 8C-4 OF 1982 CAMARO AND FIREBIRD SERVICE MANUALS) TO AVOID OBSTRUCTION OF THE HEATER FLOOR OUTLET. TRIM ANY EXCESS CARPET FROM AROUND THE DASH STUD IF NECESSARY TO ALLOW PROPER POSITIONING OF THE HUSH PANEL.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.