For 1990-2009 cars

The Universal Theft Deterrent (UDT) option UA6, combined with the remote control door lock option AU0, is available for the vehicle. The universal theft deterrent operates separately from the Personal Automotive Security System (PASS-Key II®), which is standard on the vehicle. The universal theft deterrent system is comprised of the following components:

• | The remote transmitters

• | The red security indicator lamp on the I/P upper trim panel

• | A shock sensor

• | A controller with fuel and starter disable

• | Horn outputs

• | Parking lamp outputs

• | Door jamb release switches

• | Rear lid release switches

The following actions occur for 2 minutes if a break in is attempted:

• | The system sounds the horn.

• | The parking lamps flash.

Two levels of alarm are available through the shock sensor:

• | Two horn blasts and parking lamps flash for non-threatening blows to the vehicle

• | A two-minute alarm for harder blows to the vehicle

The red lamp at the shock sensor illuminate at shock levels that would cause the full 2 minute alarm to sound.

Many of the features of the system, including the following features, can be set to the customer's preference:

• | Horn chirps

• | The method of arming the system

• | The delay times

The alarm system can be turned off. Refer to Feature Customization .