For 1990-2009 cars

# REPLACEMENT REAR COMPARTMENT NO HOLES FOR LUGGAGE COVER

WHEN THE REAR COMPARTMENT LIFT PANEL INNER COVER IS BEING REPLACED THE REPLACEMENT PANEL WILL NOT HAVE THE HOLES OR STIFFENER FOR THE LUGGAGE SHADE COVER. FOLLOWING ARE THE INSTRUCTIONS ON HOW TO CUT THE HOLES. (**SEE BULLETIN FOR ILLUSTRATION AND DETAIL INSTRUCTIONS**)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.