For 1990-2009 cars

#### Tools Required

• | J 8092 Drive Handle

• | J 26508-A Inner Output Shaft Seal Installer

• | J 21426 Outer Output Shaft Seal Installer

• | J 39546 Bearing Race Installer

• | J 39437 Bushing Installer

1. Install the mainshaft bearing race, using the J 39546 and the J 8092 .
2. Install the mainshaft bearing race retainer ring.
3. Install the output shaft seal using the J 21426 .
4. Apply sealer GM P/N United States 12346004, GM P/N Canada 10953480 or equivalent to the transmission case drain plug.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the transmission case drain plug.

Tighten
Tighten the plug to 18 N·m (13 Ib ft).