For 1990-2009 cars

### Removal Procedure

1. Open the I/P compartment door.
2. Remove the bulb from the harness connector (2).
3. Remove the retainer (1) and connector (2) from the I/P compartment, if necessary.

### Installation Procedure

1. Install the retainer (1) and connector (2) to the I/P compartment, if necessary.
2. Install the bulb to the harness connector (2).
3. Close the I/P compartment door.