For 1990-2009 cars

### Removal Procedure

1. Remove the left instrument panel insulator. Refer to Instrument Panel Insulator in Instrument Panel, Gages and Console.
2. Remove the accelerator cable (3) from the accelerator pedal lever (2).
3. Squeeze the accelerator cable cover tangs (1) and push the accelerator cable through the bulkhead.
4. Disconnect the accelerator cable from the retaining clip.
5. Disconnect the accelerator cable from the throttle body lever.
6. Disconnect the accelerator cable from the accelerator cable bracket.
7. Remove the accelerator cable.

### Installation Procedure

Notice: Do not route flexible components (hoses, wires, conduits, etc.) within 50 mm (2 in) of moving parts unless flexible components can be securely fastened. This is necessary in order to prevent possible interference and damage to the component.

1. Slide the accelerator cable (3) through the bulkhead.
2. Snap the retainer (1) through the bulkhead.
3. Connect the accelerator cable (3) through the slot in the accelerator pedal lever (2).
4. Seat the retainer (4) in the accelerator pedal lever (2).
5. Connect the accelerator cable to the throttle body lever.
6. Connect the accelerator cable to the accelerator cable bracket.
7. Connect the accelerator cable into the retaining clip.
8. Check for complete throttle opening and closing positions by operating the accelerator pedal. Also check for poor carpet fit under the accelerator pedal. The throttle should operate freely, without binding, between full closed and wide open throttle.
9. Reinstall the left instrument panel insulator. Refer to Instrument Panel Insulator in Instrument Panel, Gages and Console.