For 1990-2009 cars

## Radiator Air Baffle Assemblies and Deflectors Upper

### Removal Procedure

1. Remove the radiator air upper baffle retainers (3).
2. Remove the radiator air upper baffle (1) from the radiator (2).

### Installation Procedure

1. Install the radiator air upper baffle (1) to the radiator (2).
2. Install the radiator air upper baffle retainers (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

## Radiator Air Baffle Assemblies and Deflectors Lower

### Removal Procedure

1. Remove the air lower deflector screw (3).
2. Remove the radiator air lower baffle retainers (4).
3. Remove the radiator air lower baffle (1).
4. Inspect for any component damage.

### Installation Procedure

1. Install the radiator air lower baffle (1).
2. Install the radiator air lower baffle retainers (4).
3. Install the radiator air lower deflector screws (3).

Tighten
Tighten the screws to 10 N·m (89 lb in).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.