For 1990-2009 cars

### Assembly Procedure

1. Install the switch actuator pivot pin (2) to the pivot and pulse dimmer switch assembly (1).
2. Install the wire protector shield.
3. Align the lock housing cover and sleeve assembly (1) onto the steering column.
4. Lubricate the dimmer switch rod actuator (3) with lithium grease.
5. Install the dimmer switch rod actuator (3) to the column housing cover end base plate (2).
6. Install the column housing cover end base plate (2) to the lock housing cover and sleeve assembly (1).

Important: The bottom edge of the dimmer switch rod actuator must rest on the bend in the dimmer switch rod.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

7. Install the 3 pan head 6-lobed socket screws (1).

Tighten
Tighten the 3 pan head 6-lobed socket screws to 9 N·m (80 lb in).

8. Mount the cruise control connector (3) on the base plate (1).
9. Install the column housing cover end cap (2).
10. Install the steering column lock cylinder set. Refer to Turn Signal and Multifunction Switch Assembly - Assemble - Off Vehicle .