For 1990-2009 cars

### Removal Procedure

1. Remove the generator. Refer to Generator Replacement .
2. Remove the canister purge solenoid. Refer to Evaporative Emission Canister Purge Solenoid Valve Replacement in Engine Controls-3.8L.
3. Remove the generator rear brace bolts (5).
4. Remove the generator rear brace (4) from the vehicle.

### Installation Procedure

1. Install generator rear brace (4) to vehicle.
2. Install generator rear brace bolts.

Tighten
Tighten the generator rear brace bolts (5) to 25 N·m (18 lb ft).

3. Install the canister purge solenoid. Refer to Evaporative Emission Canister Purge Solenoid Valve Replacement in Engine Controls-3.8L.
4. Install the generator. Refer to Generator Replacement .