For 1990-2009 cars

### Removal Procedure

Important: Access to the MAP sensor is limited, but does not require removal of the intake manifold.

1. Disconnect the MAP sensor electrical connector.
2. Twist the MAP sensor forward in order to release the sensor from the retainer.
3. Pull the sensor upward.

### Installation Procedure

Important: Lightly coat the MAP sensor seal with clean engine oil before installing the sensor.

1. Install the MAP sensor. Push the MAP sensor down in order to engage the sensor into the retainer.
2. Connect the MAP sensor electrical connector.