For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Accelerator Control Cable Bracket Bolt | 10 N·m | 89 lb in
Balance Shaft Gear Bolt | 22 + 70° N·m | 16 + 70° lb ft
Balance Shaft Retainer Bolt | 30 N·m | 22 lb ft
Camshaft Position Sensor Bolt | 10 N·m | 89 lb in
Camshaft Sprocket Bolt | 100 + 90° N·m | 74 + 90° lb ft
Camshaft Thrust Plate Bolt | 15 N·m | 11 lb ft
Connecting Rod Cap Bolt | 27 + 50° N·m | 20 + 50° lb ft
Crankshaft Balancer Bolt | 150 + 114° N·m | 111 + 114° lb ft
Crankshaft Main Bearing Cap Bolt | 40 + 110° N·m | 30 + 110° lb ft
Crankshaft Main Bearing Cap Bolt (Side) | 15 + 45° N·m | 11 + 45° lb ft
Crankshaft Position Sensor Stud | 30 N·m | 22 lb ft
Crankshaft Rear Oil Seal Housing Bolt | 15 + 50° N·m | 11 + 50° lb ft
Cylinder Head Bolt | 50 + 120° N·m | 37 + 120° lb ft
Drive Belt Tensioner Bracket Bolt | 50 N·m | 37 lb ft
EGR Valve Adapter Nut | 50 N·m | 37 lb ft
EGR Valve Nut | 29 N·m | 21 lb ft
EGR Valve Outlet Pipe Bolt/Nut (Except Upper Intake Manifold) | 29 N·m | 21 lb ft
EGR Valve Wiring Harness Heat Shield Bolt/Nut | 10 N·m | 89 lb in
Engine Block Coolant Drain Plug | 18 N·m | 13 lb ft
Engine Coolant Temperature Sensor | 25 N·m | 18 lb ft
Engine Flywheel Bolt (New) | 15 + 50° N·m | 11 + 50° lb ft
Engine Front Cover Bolt/Stud | 20 + 40° N·m | 15 + 40° lb ft
Engine Lift Bracket Bolt/Nut/Stud | 30 N·m | 22 lb ft
Engine Mount Bracket Bolt | 102 N·m | 75 lb ft
Engine Mount Nut, Lower | 43 N·m | 32 lb ft
Engine Mount Nut, Upper | 47 N·m | 35 lb ft
Engine Mount Strut Bolt | 48 N·m | 35 lb ft
Engine Mount Strut Bracket Bolt at Engine, Left | 50 N·m | 37 lb ft
Engine Mount Strut Bracket Bolt at Engine, Right | 50 N·m | 37 lb ft
Engine Mount Strut Bracket Bolt at Upper Radiator Support | 28 N·m | 21 lb ft
Engine Mount Strut Nut | 48 N·m | 35 lb ft
Engine Oil Gallery Plug | 30 N·m | 22 lb ft
Exhaust Manifold Nut | 18 N·m | 13 lb ft
Exhaust Manifold Bolt/Stud | 15 N·m | 11 lb ft
Fuel Injector Rail Assembly Nut | 9 N·m | 80 lb in
Fuel Injector Rail Stud | 25 N·m | 18 lb ft
Fuel Injector Sight Shield Bracket Nut | 30 N·m | 22 lb ft
Generator Brace Bracket Bolt | 50 N·m | 37 lb ft
Heated Oxygen Sensor | 42 N·m | 31 lb ft
ICM Bracket Stud | 30 N·m | 22 lb ft
ICM Assembly Bolt/Nut | 50 N·m | 37 lb ft
Lower Intake Manifold Bolt | 15 N·m | 11 lb ft
MAP Sensor Bracket Bolt | 30 N·m | 22 lb ft
MAP Sensor Bolt | 3 N·m | 27 lb in
Oil Cooler Adapter Connector | 50 N·m | 37 lb ft
Oil Filter Adapter Bolt | 15 N·m + 50° | 11 lb ft + 50°
Oil Level Indicator Tube Nut | 19 N·m | 14 lb ft
Oil Pan Bolt | 14 N·m | 125 lb in
Oil Pan Drain Plug | 30 N·m | 22 lb ft
Oil Pump Cover Screw | 11 N·m | 98 lb in
Oil Pump Screen Bolt | 15 N·m | 11 lb ft
Power Brake Booster Heat Shield Nut | 20 N·m | 15 lb ft
Side Main Cap Bolt | 15 + 45° N·m | 11 + 45° lb ft
Starter Motor Heat Shield Bolt | 30 N·m | 22 lb ft
Throttle Body Bolt/Nut | 10 N·m | 89 lb in
Throttle Body Support Bolt | 10 N·m | 89 lb in
Timing Chain Dampener Bolt | 22 N·m | 16 lb ft
Upper Intake Manifold Bolt | Refer to Procedure
Valve Lifter Guide Retainer Bolt | 30 N·m | 22 lb ft
Valve Rocker Arm Bolt | 15 + 90° N·m | 11 + 90° lb ft
Valve Rocker Arm Cover Bolt | 10 N·m | 89 lb in
Water Outlet Bolt | 27 N·m | 20 lb ft
Water Pump Bolt | 15 + 80° N·m | 11 + 80° lb ft
Water Pump Pulley Bolt | 13 N·m | 116 lb in