For 1990-2009 cars

#### Fastener Tightening Specifications

Application | Specification
--- | ---
Metric | English
A/C Refrigerant Pressure Sensor | 6 N·m | 53 Lb In
Camshaft Position Sensor (CMP) Retaining Bolt | 10 N·m | 89 Lb In
Crankshaft Balancer Bolt | 150 N·m + 114° | 111 Lb Ft + 114°
Crankshaft Position Sensor (CKP) Bolts | 20 N·m | 15 Lb Ft
Engine Coolant Temperature Sensor (ECT) | 25 N·m | 18 Lb Ft
Engine Oil Level Switch | 20 N·m | 15 Lb Ft
Exhaust Gas Recirculation Valve (EGR) Bolts | 25 N·m | 18 Lb Ft
Fuel Filter Fitting | 30 N·m | 22 Lb Ft
Fuel Pipe Front Clip Bolt | 4.5 N·m | 40 Lb In
Fuel Pipe Rear Clip Bolt | 5.5 N·m | 49 Lb In
Fuel Pipe Shield Bolt | 5 N·m | 44 Lb In
Fuel Pipe Shield Nuts | 5 N·m | 44 Lb In
Fuel Pipe Shield Studs | 5 N·m | 44 Lb In
Fuel Rail Attaching Nuts or Bolts | 10 N·m | 89 Lb In
Fuel Sender Assembly Attaching Nuts | 6.5 N·m | 58 Lb In
Fuel Tank Retaining Strap Bolts | 33 N·m | 25 Lb Ft
Heated Oxygen Sensor | 42 N·m | 31 Lb Ft
Ignition Coil Retaining Bolts | 4.5 N·m | 40 Lb In
Ignition Control Module Retaining Bolts | 30 N·m | 22 Lb Ft
Knock Sensor | 19 N·m | 14 Lb Ft
Spark Plug | 27 N·m | 20 Lb Ft
Throttle Body Nuts or Bolts | 10 N·m | 89 Lb In