For 1990-2009 cars

#### Tools Required

• | J 8092 Drive Handle

• | J 36190 Drive Handle

• | J 39439-1 Bushing Remover

• | J 39789 Bearing Race Remover

• | J 41099 Reverse Solenoid Socket

1. Remove the reverse idler shaft bracket bolts.
2. Remove the following parts:

2.1. | The reverse idler gear thrust washer

2.2. | The reverse idler gear

2.3. | The roller bearing

2.4. | The thrust washer

2.5. | The reverse idler shaft

3. Remove the following parts:

3.1. | The countershaft extension bearing race

3.2. | The shim

3.3. | The funnel

4. Remove the following parts:

4.1. | The reverse lockout assembly bolt.

4.2. | The reverse lockout assembly

5. Remove the reverse lockout solenoid from the reverse lockout body. Use the J 41099 .

Caution: The reverse lockout assembly is under spring pressure. Exercise caution when removing the retainer ring, as bodily injury may result.

6. Disassemble the reverse lockout assembly in the following sequence:

6.1. | Refer to

#### Extension Housing (1 of 2)

(1) | Control Lever Boot
(2) | Snap Ring
(3) | Reverse Lockout
(4) | Reverse Lockout Outer Spring
(5) | Reverse Lockout Seat
(6) | Slap Ring
(7) | Reverse Lockout Inner Spring
(8) | Reverse Lockout Body
(9) | Reverse Lockout Solenoid Mounting Bolt
(10) | Reverse Lockout Solenoid
(11) | Speed sensor Bolt
(12) | Transmission Extension
(13) | Speed Sensor
(14) | Bumper
(15) | Reverse Lockout Assembly
(16) | Reverse Lockout O-Ring Seal
(17) | Bushing
(18) | Offset Shift Lever
(19) | Offset Shift Lever Pin
(20) | Isolator Cup
(21) | Shift Control Bolt
(22) | Shift Control
(23) | Shift Control Bolt

.

6.2. | Remove the O-ring (16) from the body (8).

6.3. | Remove the retainer ring (2) from the body (8).

6.4. | Remove the reverse lockout inner spring (7).

6.5. | Compress the reverse lockout plunger (3) and the collar (5) in a vise and remove the retainer ring (6).

6.6. | Remove the reverse lockout plunger (3).

6.7. | Remove the reverse lockout outer spring (4).

6.8. | Remove the reverse lockout collar (5).

7. Remove the following parts:

7.1. | The vehicle speed sensor bolt

7.2. | The vehicle speed sensor and the clamp

7.3. | The O-ring seal from the vehicle speed sensor

8. Remove the rear seal and the boot (Pry out the seal and the boot with a suitable tool).
9. Remove the mainshaft bearing race retainer ring.

Important: Do not replace the bearing race unless inspection shows bearing race damage.

10. Remove the mainshaft bearing race. Use the J 8092 and the J 39789 .

Important: Do not replace the bushing unless inspection shows bushing damage.

11. Remove the shift shaft bushing. Use the J 36190 and the J 39439-1 .