For 1990-2009 cars

Problem | Action
--- | ---
The lock system will not lock. | Inspect the lock system for the following conditions:

• | A broken or worn lock bolt spring

• | A damaged sector

• | A damaged lock cylinder

• | A burr on the lock bolt

• | A damaged housing

• | A damaged rack

• | Interference between the bowl and the rack coupling

• | A stuck ignition switch

• | A restricted actuator rod

• | An incorrectly installed sector