For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console trim plate. Refer to Console Trim Plate Replacement in Instrument Panel, Gauges, and Console.
2. Disconnect the electrical connector from shift interlock solenoid.
3. Remove the shift interlock solenoid by unsnapping the retainers.

### Installation Procedure

1. Install the shift interlock solenoid. Snap the retainers into place.
2. Connect the electrical connector to the shift interlock solenoid.
3. Install the front floor console trim plate. Refer to Console Trim Plate Replacement in Instrument Panel, Gauges, and Console.