For 1990-2009 cars

### Removal Procedure

1. Remove the washer solvent from the washer solvent container.
2. Disconnect the electrical connector from the washer pump.
3. Remove the washer pump from the washer solvent container.
4. Remove the washer hose from the washer pump.

### Installation Procedure

1. Install the washer hose on the washer pump.
2. Install the washer pump into the washer solvent container.
3. Connect the electrical connector to the washer pump.
4. Refill the washer solvent container with washer solvent.