For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION:Clutch driven plate wears rapidly.
1 | Inspect the pressure plate assembly for scoring. Is there scoring on the pressure plate assembly? | -- | Go to Step 2 | Go to Step 3
2 | Grind or replace the pressure plate assembly. Refer to Clutch Pressure and Driven Plate Replacement . Does the clutch disc still wear quickly? | -- | Go to Step 3 | System OK
3 | Inspect for weak pressure plate assembly springs. Are the pressure plate assembly springs weak? | -- | Go to Step 4 | Go to Step 5
4 | Rebuild or replace the pressure plate assembly. Refer to Clutch Pressure and Driven Plate Replacement . Does the clutch disc still wear quickly? | -- | Go to Step 5 | System OK
5 | Ride with the driver and observe his/her driving habits.m Does the driver rest his/her left foot on the clutch pedal while driving? | -- | Go to Step 6 | Go to Step 7
6 | Instruct the driver not to rest his/her foot on the clutch pedal while driving. Does the driven plate still wear quickly? | -- | Go to Step 7 | System OK
7 | Ride with the driver and observe his/her driving habits. Does the driver race the engine and slip the clutch excessively during starting? | -- | Go to Step 8 | Go to Step 9
8 | Instruct the driver not to race the engine and slip the clutch excessively during starting. Does the clutch still wear quickly? | -- | Go to Step 9 | System OK
9 | Ride with the driver and observe his/her driving habits. Does the driver hold the vehicle on hills by slipping the clutch? | -- | Go to Step 10 | --
10 | Instruct the driver not to hold the vehicle on hills by slipping the clutch. Does the clutch still wear rapidly? | -- | -- | System OK