For 1990-2009 cars

### Removal Procedure

1. Open the window panel.
2. Open the rear compartment trim, as needed. Refer to Rear Compartment Trim.
3. Disconnect the electrical connector from the switch.
4. Remove/disconnect the following components from the actuator:

• | The secondary lock retainer

• | The electrical connector

5. Remove the endgate latch. Refer to Endgate Latch Replacement .
6. Remove the bolts.
7. Remove the switch from the latch.

### Installation Procedure

1. Insert the switch to the latch.
2. Install the bolts.
3. Install the endgate latch. Refer to Endgate Latch Replacement .
4. Install/connect the following components to the actuator:

• | The secondary lock retainer

• | The electrical connector

5. Connect the electrical connector to the switch.
6. Install the rear compartment trim. Refer to Rear Compartment Trim.