For 1990-2009 cars

## Engine Mount Heat Shield Replacement 5.7L

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the engine mount heat shield nuts.
3. Remove the engine mount heat shield.

### Installation Procedure

1. Install the engine mount heat shield.
2. Install the engine mount heat shield nuts.

Tighten
Tighten the engine mount heat shield nuts to 10 N·m (89 lb in).

3. Lower the vehicle.