For 1990-2009 cars

# RATTLE NEAR 'A' PILLER AREA REPLACE PUSH-IN FASTENERS

#### SUBJECT: BUZZ OR RATTLE NEAR A-PILLAR AREA (REPLACE PUSH- IN FASTENERS AT GARNISH MOULDING AND REINSTALL)

#### VEHICLES AFFECTED: 1988-91 F CAR

#### Condition:

---------- Buzz or rattle near A-pillar area

#### Cause:

------- Garnish moulding push-in fasteners not fully seated in holes.

#### Correction:

------------ Remove garnish moulding, replace push-in fasteners P/N 363137 and reinstall making sure fasteners are fully seated.

Parts are currently available from CANSPO.

Use the most applicable Labour Operation and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.