For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 |

1. Turn the ignition to RUN with the engine OFF.
2. Disconnect the generator connector.

Does the charge indicator stay ON?

--

Go to Step 2

Go to Step 3

2 |

1. Check CKT 25 for a short to ground.
2. If OK, repair short in the driver information center flexible circuit.

Is the GEN light still on with the engine running?

--

Go to Step 3

Sytem OK

3 | Repair or replace the generator. Refer to Generator Replacement . Is the repair complete? | -- | System OK | --