For 1990-2009 cars

Perform the services shown in this schedule up to 240 000 km (150,000 miles) in this schedule and after 244 000 km (150,000 miles) at the same intervals.

#### 8 000 km (5,000 miles)

• | Change the engine oil and the filter every 12 500 km (7,500 miles) or every 12 months, whichever occurs first. An Emission Control Service *

• | Lubricate the following vehicle components when performing a maintenance schedule:

- | The steering linkage

- | The transmission shift linkage

• | Brake system inspection

• | Tire rotation

#### 25 000 km (15,000 miles)

• | Change engine oil and filter at 12 500 km (75,000 miles) or every 12 months, whichever occurs first. An Emission Control Service *

• | Lubricate the following vehicle components when performing a maintenance schedule:

- | The steering linkage

- | The transmission shift linkage

• | Brake system inspection

• | Tire rotation

#### 37 500 km (22,500 miles)

• | Change engine oil and filter every 12 500 km (7,500 miles) or every 12 months, whichever occurs first. An Emission Control Service *

• | Lubricate the following vehicle components when performing a maintenance schedule:

- | The steering linkage

- | The transmission shift linkage

• | Brake system inspection

• | Tire rotation.

#### 48 000 km (30,000 miles)

• | Change engine oil and filter every 48 000 km (30,000 miles) or every 3 months, whichever occurs first. An Emission Control Service *

• | Lubricate the following vehicle components when performing a maintenance schedule:

- | The steering linkage

- | The transmission shift linkage

• | Replace the air filters. An Emission Control Service *

• | Tire rotation

• | Inspect fuel tank, cap, and lines for damage or leaks. Inspect fuel cap gasket for any damage. Replace parts as needed.

#### 62 500 km (37,500 miles)

• | Change engine oil and filter every 12 500 km (7,500 miles) or every 12 months, whichever occurs first. An Emission Control Service *

• | Lubricate the following vehicle components when performing a maintenance schedule:

- | The steering linkage

- | The transmission shift linkage

• | Brake system inspection

• | Tire rotation

#### 72 000 km (45,000 miles)

• | Change engine oil and filter every 12 500 km (7,500 miles) or every 12 months, whichever occurs first. An Emission Control Service *

• | Lubricate the following vehicle components when performing a maintenance schedule:

- | The steering linkage

- | The transmission shift linkage

• | Brake system inspection

• | Tire rotation

#### 87 500 km (52,500 miles)

• | Change engine oil and filter every 12 500 km (7,500 miles) or every 12 months, whichever occurs first. An Emission Control Service *

• | Lubricate the following vehicle components when performing a maintenance schedule:

- | The steering linkage

- | The transmission shift linkage

• | Brake system inspection

• | Tire rotation.

#### 96 000 km (60,000 miles)

• | Change engine oil and filter every 12 500 km (7,500 miles) or every 3 months, whichever occurs first. An Emission Control Service *

• | Lubricate the following vehicle components when performing a maintenance schedule:

- | The steering linkage

- | The transmission shift linkage

• | Brake system inspection

• | Inspect serpentine drive belt

• | Replace the air filter. An Emission Control Service. *

• | Inspect fuel tank, cap, and lines for damage and replace any parts as needed.

#### 112 500 km (67,500 miles)

• | Change engine oil and filter every 12 500 km (7,500 miles) or every 12 months, whichever occurs first. An Emission Control Service *

• | Lubricate the following vehicle components when performing a maintenance schedule:

- | The steering linkage

- | The transmission shift linkage

• | Brake system inspection

• | Tire inspection

#### 120 000 km (75,000 miles)

• | Change engine oil and filter every 12 500 km (7,500 miles) or every 12 months, whichever occurs first. An Emission Control Service *

• | Lubricate the following vehicle components when performing a maintenance schedule:

- | The steering linkage

- | The transmission shift linkage

• | Brake system inspection

• | Tire rotation

#### 137 500 km (82,500 miles)

• | Change engine oil and filter every 12 500 km (7,500 miles) or every 12 months, or whichever occurs first. An Emission Control Service *

• | Lubricate the following vehicle components when performing a maintenance schedule:

- | The steering linkage

- | The transmission shift linkage

• | Tire rotation.

#### 144 000 km (90,000 miles)

• | Change engine oil and filter every 12,000 km (7,500 miles) or every 12 months, whichever occurs first. An Emission Control Service *

• | Lubricate the following vehicle components when performing a maintenance schedule:

- | The steering linkage

- | The transmission shift linkage

• | Replace the air filter. An Emission Control Service.

• | Tire rotation

• | Brake system inspection

• | Inspect fuel tank, cap, and lines for damage or leaks. Inspect cap gasket for any damage and replace parts as necessary.

#### 162 500 km (97,500 miles)

• | Change engine oil and filter every 12 000 km (7,500 miles) or every 12 months, whichever occurs first. An Emission Control Service *

• | Lubricate the following vehicle components when performing a maintenance schedule:

- | The steering linkage

- | The transmission shift linkage

• | Brake system inspection

• | Tire rotation

#### 160 000 km (100,000 miles)

• | Inspect spark plug wires.

• | Replace spark plugs

• | Rotate the tire. Refer to Tire Rotation in Tires and Wheels.

• | Change the automatic transmission fluid and filter.

#### 240 000 km (150,000 miles)

• | Drain, flush and refill the cooling system every 240 000 km (150,000 miles ) or every 60 months, whatever exceeds first. Refer to Fluid and Lubricant Recommendations in General Information. Inspect the hoses. Clean the radiator, condenser, pressure cap and neck. An Emission Control Service *

• | Inspect hoses

• | Clean radiator, condensor, pressure cap and neck.

• | Pressure test cooling system and pressure cap.