For 1990-2009 cars

# RATTLE NEAR 'A' PILLER AREA REPLACE PUSH-IN FASTENERS

#### Subject: BUZZ OR RATTLE NEAR A-PILLAR AREA (REPLACE PUSH-IN FASTENERS AT GARNISH MOLDING AND REINSTALL)

#### Models Affected: 1988-91 FIREBIRD MODELS

Condition: Buzz or rattle near A-pillar area

Cause: Garnish molding push-in fasteners not fully seated in holes.

Correction: Remove garnish molding, replace push-in fasteners P/N 363137 and reinstall making sure fasteners are fully seated.

Parts are currently available from GMSPO.

Labor Operation Number: Labor Time: ----------------------- ----------- Left Side C2011 0.3 Hours

Right Side C2010 0.3 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.