For 1990-2009 cars

### Removal Procedure

1. Disconnect the main electrical connector feeding the ignition coils.
2. Disconnect the ignition coil harness connector.
3. Disconnect the spark plug wire at the ignition coil.
4. Remove the ignition coil mounting bolts.
5. Remove the ignition coil.

### Installation Procedure

1. Install the ignition coil.
2. Install the ignition coil mounting bolts.

Tighten
Tighten the Ignition coil mounting bolts to 12 N·m (106 lb in).

3. Connect the spark plug wire at the ignition coil.
4. Connect the ignition coil harness connector.
5. Connect the main electrical connector feeding the ignition coils.