For 1990-2009 cars

Clean any corrosion from the battery tray/coolant recovery reservoir and the hold down clamp prior to installing the battery. Ensure the carrier is in good condition in order to hold the battery securely and keep the battery level. Ensure there are no parts or tools in the battery tray/coolant recovery reservoir before installing the battery. In order to prevent the battery from shaking in the tray, tighten the hold down bolt to the specification noted. Refer to Fastener Tightening Specifications