For 1990-2009 cars

1. Apply an evenly distributed load to the clutch pack.
2. Apply medium pressure.

Tighten
Tighten approximately 89 N·m (20 lb ft), on the selective backing plate.

3. Use feeler gages to check the reverse input clutch plate travel.
4. Check the travel between the selective backing plate and the reverse input clutch retainer ring.

The reverse input clutch plate travel should be 1.02-1.94 mm (0.040-0.076 in).

5. Select the proper selective backing plate to obtain the correct travel. Refer to Reverse Input Clutch Backing Plate Selection .