For 1990-2009 cars

## Shoulder Restraint Guide Replacement - Rear Seat Standard

### Removal Procedure

1. Remove the bolts (2) that attach the guide (1) to the rear seatback cushion.
2. Remove the guide (1).

### Installation Procedure

1. Install the guide (1) to the rear seatback cushion.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts (2).

Tighten
Tighten the bolts to 10 N·m (89 lb in).

## Shoulder Restraint Guide Replacement - Rear Seat Convertible

### Removal Procedure

1. Remove the bolts (1) that attach the guide (2) to the rear seatback cushion.
2. Remove the guide (2).

### Installation Procedure

1. Install the guide (2) to the rear seatback cushion.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts (1).

Tighten
Tighten the bolts (1) to 10 N·m (89 lb in).